MID accessory set without adapter piece,
consisting of 2 x locking valves,
temperature-measuring ball valve for
sensor integration, directly submersible.
DN:  20

Manufacturer: Belimo
Type: EXT-EF-20A